The HMS POWERLINK XDDFile Uploader only works with firmware version 1.05 or later

Scan Procedure:
1. use a alone network port for the powerlink slave.
2. start HMS POWERLINK XDDFile Uploader
3. disconnect network cable from slave, the press start scan.
4. wait until status show: resetting network, then connect network cable
   (if not doing so, the software will stop, saying that there are traffic in the line)
5. the soft will continue searching for slaves.
6. knowing the node address, wait until it reaches the number, stop the scan.
7. press "upload XDD file", give the destination filename and wait it to finish.


