EPSG POWERLINK-Office Bonsaiweg 6 15370 Fredersdorf, Germany Phone: +49 33439 539 270 Fax: +49 33439 539 272 info@ethernet-powerlink.org www.ethernet-powerlink.org |

## Conformance-Test Report

### Test-Execution

Created by: | burreinerw
Created on: | 2017-02-08, 08:49:36 UTC
Filename: | C:\Users\burreinerw\Documents\Certification 07.02.2017\Dina\Advanced_Tests\FFFF000F_DinaSL-VarioPowerLink_TestResults.xml

### Device

Vendor name: | Dina Elektronik
Vendor id: | 0xFFFF000F
Product name: | Dina SL-Vario PowerLink
Product id: | N/A
SW-Version: | N/A
HW-Version: | FBV 4.3/AB6711
FW-Version: | 1.07.01
Serial number: | N/A

### XDD

Filename: | FFFF000F_DinaSL-VarioPowerLink.xdd
Created on: | 2016-05-20
Modified on: | N/A
Version: | 1.07.01

### Test-Environment

openCONFORMANCE version: | 1.3.2
EPSG DS301 Communication Profile version: | 1.2.0
EPSG DS301 Communication Profile date: | 2013-12-17
EPSG DS310 Conformance-Test Specification version: | 1.0.7
EPSG DS310 Conformance-Test Specification date: | 2013-02-28
Managing Node stack-type: | openPOWERLINK
Managing Node stack-version: | 1.8.5 adapted
Managing Node stack-date: | 2014-09-04
Managing Node cycle-time[µs]: | 50000

### Test-Statistics

Overall Testresult: | PASSED
Statistics: | 0/20 FAILED, 14/20 PASSED, 6/20 NOT_SUPPORTED

### Test-Results

Testcase: Testcase_3_3_1_1_T1 | Testgroup: ERROR_BEHAVIOR_TESTS | Teststate: COMPLETED | Testresult: PASSED
Error: E3_3_1_1_T1_F3
Severity: WARN
Cumulative counter invalid. Cumulative counter (0x1C0B/0x1) invalid (must not be reset by NMT reset-commands). Actual value: 0 Expected value: 2

Testcase: Testcase_3_3_1_1_T2 | Testgroup: ERROR_BEHAVIOR_TESTS | Teststate: COMPLETED | Testresult: PASSED

Testcase: Testcase_3_3_1_1_T3 | Testgroup: ERROR_BEHAVIOR_TESTS | Teststate: COMPLETED | Testresult: NOT_SUPPORTED
Error: E3_3_1_1_T3_F7
Severity: INFO
Error-Handling not supported. Device-XDD states that error-handling (object 0x1C0C) is not supported for this error-source.

Testcase: Testcase_3_3_1_1_T4 | Testgroup: ERROR_BEHAVIOR_TESTS | Teststate: COMPLETED | Testresult: NOT_SUPPORTED
Error: E3_3_1_1_T4_F3
Severity: INFO
Error-Handling not supported. Device-XDD states that error-handling (object 0x1C0C) is not supported for this error-source.

Testcase: Testcase_3_3_1_1_T5 | Testgroup: ERROR_BEHAVIOR_TESTS | Teststate: COMPLETED | Testresult: NOT_SUPPORTED
Error: E3_3_1_1_T5_F7
Severity: INFO
Error-Handling not supported. Device-XDD states that error-handling (object 0x1C0D) is not supported for this error-source.

Testcase: Testcase_3_3_1_1_T6 | Testgroup: ERROR_BEHAVIOR_TESTS | Teststate: COMPLETED | Testresult: NOT_SUPPORTED
Error: E3_3_1_1_T6_F3
Severity: INFO
Error-Handling not supported. Device-XDD states that error-handling (object 0x1C0D) is not supported for this error-source.

Testcase: Testcase_3_3_1_1_T7 | Testgroup: ERROR_BEHAVIOR_TESTS | Teststate: COMPLETED | Testresult: PASSED
Error: E3_3_1_1_T7_F2
Severity: WARN
Cumulative counter invalid. Cumulative counter (0x1C0B/0x1) invalid. Actual value: 1 Expected value: 2

Testcase: Testcase_3_3_1_1_T8 | Testgroup: ERROR_BEHAVIOR_TESTS | Teststate: COMPLETED | Testresult: NOT_SUPPORTED
Error: E3_3_1_1_T8_F4
Severity: INFO
Error-Handling not supported. Device-XDD states that error-handling (object 0x1C0C) is not supported for this error-source.

Testcase: Testcase_3_3_1_1_T9 | Testgroup: ERROR_BEHAVIOR_TESTS | Teststate: COMPLETED | Testresult: NOT_SUPPORTED
Error: E3_3_1_1_T9_F4
Severity: INFO
Error-Handling not supported. Device-XDD states that error-handling (object 0x1C0C) is not supported for this error-source.

Testcase: Testcase_3_3_1_3_T1 | Testgroup: EXT_COMP_TESTS | Teststate: COMPLETED | Testresult: PASSED

Testcase: Testcase_3_3_1_3_T2 | Testgroup: EXT_COMP_TESTS | Teststate: COMPLETED | Testresult: PASSED

Testcase: Testcase_3_3_1_3_T3 | Testgroup: EXT_COMP_TESTS | Teststate: COMPLETED | Testresult: PASSED

Testcase: Testcase_3_3_1_4_T1 | Testgroup: ERROR_BEHAVIOR_TESTS | Teststate: COMPLETED | Testresult: PASSED

Testcase: Testcase_3_3_1_4_T10 | Testgroup: ERROR_BEHAVIOR_TESTS | Teststate: COMPLETED | Testresult: PASSED

Testcase: Testcase_3_3_1_4_T2 | Testgroup: ERROR_BEHAVIOR_TESTS | Teststate: COMPLETED | Testresult: PASSED

Testcase: Testcase_3_3_1_4_T4 | Testgroup: ERROR_BEHAVIOR_TESTS | Teststate: COMPLETED | Testresult: PASSED
Error: E3_3_1_4_T4_F1
Severity: WARN
Correctly addressed ASnd-Frame not interpreted. CN did not change its state from CS_OPERATIONAL to CS_STOPPED on reception of NMTStopNode command with destination MAC-Address FF:FF:FF:FF:FF:FF and destination nodeId 0x01.

Testcase: Testcase_3_3_1_4_T5 | Testgroup: ERROR_BEHAVIOR_TESTS | Teststate: COMPLETED | Testresult: PASSED
Error: E3_3_1_4_T5_F1
Severity: WARN
Correctly addressed ASnd-Frame not interpreted. CN did not change its state from CS_OPERATIONAL to CS_STOPPED on reception of NMTStopNode command with destination MAC-Address FF:FF:FF:FF:FF:FF and destination nodeId 0xFF.

Testcase: Testcase_3_3_1_4_T6 | Testgroup: ERROR_BEHAVIOR_TESTS | Teststate: COMPLETED | Testresult: PASSED

Testcase: Testcase_3_3_1_4_T7 | Testgroup: ERROR_BEHAVIOR_TESTS | Teststate: COMPLETED | Testresult: PASSED

Testcase: Testcase_3_3_1_4_T9 | Testgroup: ERROR_BEHAVIOR_TESTS | Teststate: COMPLETED | Testresult: PASSED