EPSG POWERLINK-Office Bonsaiweg 6 15370 Fredersdorf, Germany Phone: +49 33439 539 270 Fax: +49 33439 539 272 info@ethernet-powerlink.org www.ethernet-powerlink.org |

## Conformance-Test Report

### Test-Execution

Created by: | burreinerw
Created on: | 2017-02-08, 08:42:12 UTC
Filename: | C:\Users\burreinerw\Documents\Certification 07.02.2017\Dina\Basic_Tests\FFFF000F_DinaSL-VarioPowerLink_TestResults.xml

### Device

Vendor name: | Dina Elektronik
Vendor id: | 0xFFFF000F
Product name: | Dina SL-Vario PowerLink
Product id: | N/A
SW-Version: | N/A
HW-Version: | FBV 4.3/AB6711
FW-Version: | 1.07.01
Serial number: | N/A

### XDD

Filename: | FFFF000F_DinaSL-VarioPowerLink.xdd
Created on: | 2016-05-20
Modified on: | N/A
Version: | 1.07.01

### Test-Environment

openCONFORMANCE version: | 1.3.2
EPSG DS301 Communication Profile version: | 1.2.0
EPSG DS301 Communication Profile date: | 2013-12-17
EPSG DS310 Conformance-Test Specification version: | 1.0.7
EPSG DS310 Conformance-Test Specification date: | 2013-02-28
Managing Node stack-type: | openPOWERLINK
Managing Node stack-version: | 1.8.5 adapted
Managing Node stack-date: | 2014-09-04
Managing Node cycle-time[µs]: | 50000

### Test-Statistics

Overall Testresult: | PASSED
Statistics: | 0/62 FAILED, 31/62 PASSED, 31/62 NOT_SUPPORTED

### Test-Results

Testcase: Testcase_3_2_1_T1 | Testgroup: BOOTUP_TESTS | Teststate: COMPLETED | Testresult: PASSED

Testcase: Testcase_3_2_1_T2 | Testgroup: BOOTUP_TESTS | Teststate: COMPLETED | Testresult: PASSED

Testcase: Testcase_3_2_2_T1 | Testgroup: BOOTUP_TESTS | Teststate: COMPLETED | Testresult: PASSED

Testcase: Testcase_3_2_3_T1 | Testgroup: BOOTUP_TESTS | Teststate: COMPLETED | Testresult: PASSED

Testcase: Testcase_3_2_3_T2 | Testgroup: BOOTUP_TESTS | Teststate: COMPLETED | Testresult: PASSED

Testcase: Testcase_3_2_4_T1 | Testgroup: BOOTUP_TESTS | Teststate: COMPLETED | Testresult: PASSED

Testcase: Testcase_3_2_4_T3 | Testgroup: BOOTUP_TESTS | Teststate: COMPLETED | Testresult: PASSED

Testcase: Testcase_3_2_5_T1 | Testgroup: BOOTUP_TESTS | Teststate: COMPLETED | Testresult: PASSED

Testcase: Testcase_3_2_5_T2 | Testgroup: BOOTUP_TESTS | Teststate: COMPLETED | Testresult: PASSED

Testcase: Testcase_3_2_6_T1 | Testgroup: BASIC_SDO_TESTS | Teststate: COMPLETED | Testresult: PASSED

Testcase: Testcase_3_2_6_T10_1 | Testgroup: BASIC_SDO_TESTS | Teststate: COMPLETED | Testresult: PASSED

Testcase: Testcase_3_2_6_T2_1 | Testgroup: BASIC_SDO_TESTS | Teststate: COMPLETED | Testresult: PASSED

Testcase: Testcase_3_2_6_T2_2 | Testgroup: BASIC_SDO_TESTS | Teststate: COMPLETED | Testresult: NOT_SUPPORTED
Error: E3_2_6_T2_2_F1
Severity: INFO
Ident-Response of CN indicates that SDO by UDP is not supported. No additional info provided.

Testcase: Testcase_3_2_6_T2_3 | Testgroup: BASIC_SDO_TESTS | Teststate: COMPLETED | Testresult: NOT_SUPPORTED
Error: E3_2_6_T2_3_F1
Severity: INFO
Ident-Response of CN indicates that SDO by PDO is not supported. No additional info provided.

Testcase: Testcase_3_2_6_T3_1 | Testgroup: BASIC_SDO_TESTS | Teststate: COMPLETED | Testresult: PASSED

Testcase: Testcase_3_2_6_T4_1 | Testgroup: BASIC_SDO_TESTS | Teststate: COMPLETED | Testresult: PASSED

Testcase: Testcase_3_2_6_T5_1 | Testgroup: BASIC_SDO_TESTS | Teststate: COMPLETED | Testresult: PASSED

Testcase: Testcase_3_2_6_T6_1 | Testgroup: BASIC_SDO_TESTS | Teststate: COMPLETED | Testresult: PASSED

Testcase: Testcase_3_2_6_T8_1 | Testgroup: BASIC_SDO_TESTS | Teststate: COMPLETED | Testresult: PASSED

Testcase: Testcase_3_2_6_T9_1 | Testgroup: BASIC_SDO_TESTS | Teststate: COMPLETED | Testresult: PASSED

Testcase: Testcase_3_2_7_T2_1 | Testgroup: NMT_STATE_CMD_TESTS | Teststate: COMPLETED | Testresult: PASSED

Testcase: Testcase_3_2_7_T2_2 | Testgroup: NMT_STATE_CMD_TESTS | Teststate: COMPLETED | Testresult: PASSED

Testcase: Testcase_3_2_7_T3_1 | Testgroup: NMT_STATE_CMD_TESTS | Teststate: COMPLETED | Testresult: NOT_SUPPORTED
Error: E3_2_7_T3_1_F4
Severity: INFO
Featureflags (XDD) indicate that extended NMT-State commands are not supported. No additional info provided.

Testcase: Testcase_3_2_7_T3_2 | Testgroup: NMT_STATE_CMD_TESTS | Teststate: COMPLETED | Testresult: NOT_SUPPORTED
Error: E3_2_7_T3_2_F4
Severity: INFO
Featureflags (XDD) indicate that extended NMT-State commands are not supported. No additional info provided.

Testcase: Testcase_3_2_7_T3_3 | Testgroup: NMT_STATE_CMD_TESTS | Teststate: COMPLETED | Testresult: NOT_SUPPORTED
Error: E3_2_7_T3_3_F4
Severity: INFO
Featureflags (XDD) indicate that extended NMT-State commands are not supported. No additional info provided.

Testcase: Testcase_3_2_7_T4 | Testgroup: NMT_STATE_CMD_TESTS | Teststate: COMPLETED | Testresult: NOT_SUPPORTED
Error: E3_2_7_T4_F4
Severity: INFO
Featureflags (XDD) indicate that extended NMT-State commands are not supported. No additional info provided.

Testcase: Testcase_3_2_7_T5_1 | Testgroup: NMT_STATE_CMD_TESTS | Teststate: COMPLETED | Testresult: PASSED

Testcase: Testcase_3_2_7_T5_2 | Testgroup: NMT_STATE_CMD_TESTS | Teststate: COMPLETED | Testresult: NOT_SUPPORTED
Error: E3_2_7_T5_2_F4
Severity: INFO
Featureflags (XDD) indicate that extended NMT-State commands are not supported. No additional info provided.

Testcase: Testcase_3_2_9_T1 | Testgroup: OD_READ_TESTS | Teststate: COMPLETED | Testresult: PASSED

Testcase: Testcase_3_2_9_T10_1 | Testgroup: OD_BEHAVIOR_TESTS | Teststate: COMPLETED | Testresult: NOT_SUPPORTED
Error: E3_2_9_T10_1_F7
Severity: INFO
Featureflags (XDD) indicate that extended NMT-State commands are not supported. No additional info provided.

Testcase: Testcase_3_2_9_T10_2 | Testgroup: OD_BEHAVIOR_TESTS | Teststate: COMPLETED | Testresult: NOT_SUPPORTED
Error: E3_2_9_T10_2_F7
Severity: INFO
Featureflags (XDD) indicate that extended NMT-State commands are not supported. No additional info provided.

Testcase: Testcase_3_2_9_T10_3 | Testgroup: OD_BEHAVIOR_TESTS | Teststate: COMPLETED | Testresult: NOT_SUPPORTED
Error: E3_2_9_T10_3_F7
Severity: INFO
Featureflags (XDD) indicate that extended NMT-State commands are not supported. No additional info provided.

Testcase: Testcase_3_2_9_T10_4 | Testgroup: OD_BEHAVIOR_TESTS | Teststate: COMPLETED | Testresult: NOT_SUPPORTED
Error: E3_2_9_T10_4_F7
Severity: INFO
Featureflags (XDD) indicate that extended NMT-State commands are not supported. No additional info provided.

Testcase: Testcase_3_2_9_T2 | Testgroup: OD_WRITE_TESTS | Teststate: COMPLETED | Testresult: PASSED

Testcase: Testcase_3_2_9_T3_1 | Testgroup: OD_WRITE_TESTS | Teststate: COMPLETED | Testresult: PASSED

Testcase: Testcase_3_2_9_T3_2 | Testgroup: OD_WRITE_TESTS | Teststate: COMPLETED | Testresult: PASSED

Testcase: Testcase_3_2_9_T3_3 | Testgroup: OD_WRITE_TESTS | Teststate: COMPLETED | Testresult: PASSED

Testcase: Testcase_3_2_9_T3_4 | Testgroup: OD_WRITE_TESTS | Teststate: COMPLETED | Testresult: PASSED

Testcase: Testcase_3_2_9_T4_1 | Testgroup: OD_STORE_TESTS | Teststate: COMPLETED | Testresult: NOT_SUPPORTED
Error: E3_2_9_T4_1_F1
Severity: INFO
Device does not support storage of parameters. Device-XDD does not contain object 0x1010 (storage of parameters).

Testcase: Testcase_3_2_9_T4_2 | Testgroup: OD_STORE_TESTS | Teststate: COMPLETED | Testresult: NOT_SUPPORTED
Error: E3_2_9_T4_2_F1
Severity: INFO
Device does not support storage of parameters. Device-XDD does not contain object 0x1010 (storage of parameters).

Testcase: Testcase_3_2_9_T5_1 | Testgroup: OD_STORE_TESTS | Teststate: COMPLETED | Testresult: NOT_SUPPORTED
Error: E3_2_9_T5_1_F1
Severity: INFO
Device does not support storage of parameters. Device-XDD does not contain object 0x1010 (storage of parameters).

Testcase: Testcase_3_2_9_T5_2 | Testgroup: OD_STORE_TESTS | Teststate: COMPLETED | Testresult: NOT_SUPPORTED
Error: E3_2_9_T5_2_F1
Severity: INFO
Device does not support storage of parameters. Device-XDD does not contain object 0x1010 (storage of parameters).

Testcase: Testcase_3_2_9_T5_3 | Testgroup: OD_STORE_TESTS | Teststate: COMPLETED | Testresult: NOT_SUPPORTED
Error: E3_2_9_T5_3_F1
Severity: INFO
Device does not support storage of parameters. Device-XDD does not contain object 0x1010 (storage of parameters).

Testcase: Testcase_3_2_9_T5_4 | Testgroup: OD_STORE_TESTS | Teststate: COMPLETED | Testresult: NOT_SUPPORTED
Error: E3_2_9_T5_4_F1
Severity: INFO
Device does not support storage of parameters. Device-XDD does not contain object 0x1010 (storage of parameters).

Testcase: Testcase_3_2_9_T5_5 | Testgroup: OD_STORE_TESTS | Teststate: COMPLETED | Testresult: NOT_SUPPORTED
Error: E3_2_9_T5_5_F1
Severity: INFO
Device does not support storage of parameters. Device-XDD does not contain object 0x1010 (storage of parameters).

Testcase: Testcase_3_2_9_T5_6 | Testgroup: OD_STORE_TESTS | Teststate: COMPLETED | Testresult: NOT_SUPPORTED
Error: E3_2_9_T5_6_F1
Severity: INFO
Device does not support storage of parameters. Device-XDD does not contain object 0x1010 (storage of parameters).

Testcase: Testcase_3_2_9_T5_7 | Testgroup: OD_STORE_TESTS | Teststate: COMPLETED | Testresult: NOT_SUPPORTED
Error: E3_2_9_T5_7_F1
Severity: INFO
Device does not support storage of parameters. Device-XDD does not contain object 0x1010 (storage of parameters).

Testcase: Testcase_3_2_9_T5_8 | Testgroup: OD_STORE_TESTS | Teststate: COMPLETED | Testresult: NOT_SUPPORTED
Error: E3_2_9_T5_8_F1
Severity: INFO
Device does not support storage of parameters. Device-XDD does not contain object 0x1010 (storage of parameters).

Testcase: Testcase_3_2_9_T6_1 | Testgroup: OD_RESTORE_TESTS | Teststate: COMPLETED | Testresult: NOT_SUPPORTED
Error: E3_2_9_T6_1_F1
Severity: INFO
Device does not support store or restore of parameters. Device-XDD does not contain object 0x1010 (storage of parameters) or 0x1011 (restore of parameters).

Testcase: Testcase_3_2_9_T6_2 | Testgroup: OD_RESTORE_TESTS | Teststate: COMPLETED | Testresult: NOT_SUPPORTED
Error: E3_2_9_T6_2_F1
Severity: INFO
Device does not support store or restore of parameters. Device-XDD does not contain object 0x1010 (storage of parameters) or 0x1011 (restore of parameters).

Testcase: Testcase_3_2_9_T7_1 | Testgroup: OD_RESTORE_TESTS | Teststate: COMPLETED | Testresult: NOT_SUPPORTED
Error: E3_2_9_T7_1_F1
Severity: INFO
Device does not support store or restore of parameters. Device-XDD does not contain object 0x1010 (storage of parameters) or 0x1011 (restore of parameters).

Testcase: Testcase_3_2_9_T7_2 | Testgroup: OD_RESTORE_TESTS | Teststate: COMPLETED | Testresult: NOT_SUPPORTED
Error: E3_2_9_T7_2_F1
Severity: INFO
Device does not support store or restore of parameters. Device-XDD does not contain object 0x1010 (storage of parameters) or 0x1011 (restore of parameters).

Testcase: Testcase_3_2_9_T7_3 | Testgroup: OD_RESTORE_TESTS | Teststate: COMPLETED | Testresult: NOT_SUPPORTED
Error: E3_2_9_T7_3_F1
Severity: INFO
Device does not support store or restore of parameters. Device-XDD does not contain object 0x1010 (storage of parameters) or 0x1011 (restore of parameters).

Testcase: Testcase_3_2_9_T7_4 | Testgroup: OD_RESTORE_TESTS | Teststate: COMPLETED | Testresult: NOT_SUPPORTED
Error: E3_2_9_T7_4_F1
Severity: INFO
Device does not support store or restore of parameters. Device-XDD does not contain object 0x1010 (storage of parameters) or 0x1011 (restore of parameters).

Testcase: Testcase_3_2_9_T7_5 | Testgroup: OD_RESTORE_TESTS | Teststate: COMPLETED | Testresult: NOT_SUPPORTED
Error: E3_2_9_T7_5_F1
Severity: INFO
Device does not support store or restore of parameters. Device-XDD does not contain object 0x1010 (storage of parameters) or 0x1011 (restore of parameters).

Testcase: Testcase_3_2_9_T7_6 | Testgroup: OD_RESTORE_TESTS | Teststate: COMPLETED | Testresult: NOT_SUPPORTED
Error: E3_2_9_T7_6_F1
Severity: INFO
Device does not support store or restore of parameters. Device-XDD does not contain object 0x1010 (storage of parameters) or 0x1011 (restore of parameters).

Testcase: Testcase_3_2_9_T7_7 | Testgroup: OD_RESTORE_TESTS | Teststate: COMPLETED | Testresult: NOT_SUPPORTED
Error: E3_2_9_T7_7_F1
Severity: INFO
Device does not support store or restore of parameters. Device-XDD does not contain object 0x1010 (storage of parameters) or 0x1011 (restore of parameters).

Testcase: Testcase_3_2_9_T7_8 | Testgroup: OD_RESTORE_TESTS | Teststate: COMPLETED | Testresult: NOT_SUPPORTED
Error: E3_2_9_T7_8_F1
Severity: INFO
Device does not support store or restore of parameters. Device-XDD does not contain object 0x1010 (storage of parameters) or 0x1011 (restore of parameters).

Testcase: Testcase_3_2_9_T9_1 | Testgroup: OD_BEHAVIOR_TESTS | Teststate: COMPLETED | Testresult: PASSED

Testcase: Testcase_3_2_9_T9_2 | Testgroup: OD_BEHAVIOR_TESTS | Teststate: COMPLETED | Testresult: PASSED

Testcase: Testcase_3_2_9_T9_3 | Testgroup: OD_BEHAVIOR_TESTS | Teststate: COMPLETED | Testresult: PASSED

Testcase: Testcase_3_2_9_T9_4 | Testgroup: OD_BEHAVIOR_TESTS | Teststate: COMPLETED | Testresult: PASSED